**Chapter 222 Swimming Pools, Spas and Hot Tubs**

**222-1 Definitions**

[**SWIMMING POOL**](http://www.ecode360.com/5124369#5124369)

Any body of water (excluding natural bodies of water fed by rivers, streams or brooks) or receptacle for water that is capable of having a depth at any point greater than two feet used or intended to be used for swimming or bathing and constructed, installed or maintained in or above the ground outside or inside any building. *This also includes hot tubs and spas*

**222-2 Requirements**

B. Safety measures. Any such pool shall be completely enclosed by a *barrier* not less than four feet in height, with all gates or doors opening through such enclosure equipped with self-closing and self-latching devices designed to keep and capable of keeping such gates or doors securely closed at all times when not in actual use, of a type approved by the Code Enforcement Officer. *The barrier shall consist of a fence, a wall, a building, or any combination thereof.*